laser

### Performing a Linear Open Advanced Scan

Linear Open Scan dialog box

The Linear Open Scan method scans the surface along a line. This procedure uses the starting and ending points for the line, and also includes a direction point for the calculation of the cut plane. The probe always remains within the cut plane while doing the scan.

The topics for a Linear Open Advanced scan include:

- To Create a Linear Open Scan

- Linear Open Scan Parameters

- Vectors

More:

Using the Simulate Pointcloud Function