laser

#### Flush and Gap Command Mode Text

The Flush and Gap command inside the Edit window’s Command Mode looks like this:

FNG2 =FEAT/LASER/FLUSH AND GAP/DEFAULT,CARTESIAN

THEO/<124.012,13.241,0>,<0,0,1>,<1,0,0>,0,7.985

ACTL/<124.012,13.241,0>,<0,0,1>,<1,0,0>,0,7.985

TARG/<124.012,13.241,0>,<0,0,1>

MASTER SIDE POINT

THEO/<128,13.241,0>,<0,0,1>

ACTL/<0,0,0>,<0,0,0>

GAUGE SIDE POINT

THEO/<120,13.241,0>,<0,0,1>

ACTL/<0,0,0>,<0,0,0>

CUT PLANE VECTOR<0,1,0>,<0,1,0>

Depth=1

INDENT=3

SPACER=1.5

SHOW FEATURE PARAMETERS=NO

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

ZOOM=2A,GAIN=NORMAL,OVERLAP=1

OVERSCAN=5

REDUCTION FILTER=OFF

FILTER LINES=Disabled

CLIPPING TOP=100,BOTTOM=0,LEFT=0,RIGHT=100

SOUND=ON

HORIZONTAL CLIPPING=2,VERTICAL CLIPPING=5