cmm

#### Axis Basic Scan - Type Values Method

Use this method to type the X, Y, and Z values of the start and end points for an axis basic scan.

1. Double-click on the desired point in the # column in the BASICSCAN dialog box (Insert | Scan | Axis). The Edit Scan Item dialog box appears:

Edit Scan Item dialog box

The title bar of the dialog box displays the ID of the specific parameter being edited.

2. Edit the X, Y, and Z values.

3. To apply your changes, click OK. To cancel your changes and close the dialog box, click Cancel.

4. Use this same procedure to edit the CutVec and InitVec values of the axis.

For more information about the BASICSCAN dialog box and the axis basic scan, see "Performing an Axis Basic Scan".