settingseditor

### ClientIsHolos

This registry entry specifies bit-coded values that perform the following operations:

- Bit 0 (value 1) = Does not send or use the A0B0 angle. Also forces the UseWristStrategy registry entry to be set for the ToolName registry entry if a wrist device is involved.

- Bit 1 (value 2) = Forces the system to not send or use A0B0 angle for the ToolName registry entry. It is independent of whether or not a wrist device is used. It also forces the UseWristStrategy registry entry to be set.

- Bit 2 (value 4) = Prevents sending E-Stops or similar code 8000 by dozens if machine remains in E-Stop state, or error reoccurs every second.

- Bit 4 (value 8) = Introduces a delay (in ms) of the value for the HolosSlowDown registry entry before sending ACK (&) / END (%)/error answer.

Entry Name: ClientIsHolos

Entry Type: Bit-coded integers of 0 (zero), 1, 2, or 4. The default value is 0.