core

#### Calibrating the LSPX5 / HR-XS Probe Changer

The calibration process for the LSPX5 / HR-XS probe changer represents the steps that you would take to prepare to use any of the probe changers that PC-DMIS supports. The process discussed here is specific to the LSPX5 / HR-XS Probe Changer.

The LSPX5 / HR-XS probe changer needs to be mounted on the machine table parallel to either the X or Y axis. For mounting instructions, consult the documentation that came with your probe changer.

LSPX5 / HR-XS Probe Changer

To calibrate your probe changer:

Step 1 - Select the LSPX5 / HR-XS Probe Changer

Step 2 - Define the Mount Point

Step 3 - Define the Number of Ports

Step 4 - Prepare for Calibration

Step 5 - Take a Point with the Over-Hang of the Collet

Step 6 - Define the Location of the First Port

Step 7 - Define the Location of the Second Port