core

### Step 9: Calibrate the Multiple Arm Probe Files

Now that the system has been calibrated, you need to calibrate the multiple arm probe files.

For this calibration, you can:

- Calibrate any arm in any order.

- Use different calibration tools to calibrate the different arms.

- Calibrate Arm2 from the Arm2 computer and Arm1 from the Arm1 computer.

- Calibrate the Arm2 probe on the same calibration tool as the Arm1 probe.

- Only calibrate one arm at a time.

After this calibration, PC-DMIS synchronizes the probe files from the multiple computers the next time you enter multiple arm mode on the Arm1 computer.

- Arm 1 Probe File Calibration

- Arm 2 Probe File Calibration

Next Step