miim

### MP-533 No amp/check/divide board present

The SMP-400 requires that an amp/check/divide card be present at the base address. The amp/check/divide card may have failed or may be set to the wrong address.

For more information, see "MP Error Codes".

What you should do:

1. Note the error data that is displayed on the SMP-400 diagnostic LED.

2. If the error reoccurs, contact your Giddings & Lewis service representative.