miim

### MP-565 UART interrupt failure

On an SMP-400 system, interrupt generated on electronic level UART but not received by the interrupt controller chip on the processor board.

For more information, see "MP Error Codes".

What you should do:

1. Note the error data that is displayed on the SMP-400 internal diagnostic LED.

2. If the error reoccurs, contact your Giddings & Lewis service representative.