miim

### Installation Information

Installing PC-DMIS with a portlock or an LMS license that is correctly configured for the FDC-VisionBox interface ensures that the correct files and registry entries are set up during the installation.

The license requires the following:

- Vision - Enabled

- Interface - Vision

- Vision Type - Vision Box

- Laser Probe Type - If required: Mycrona WLS in case of CWS / Mycrona TTL in case of TTL

Additional requirements:

- Vision Frame Grabber should already be installed. For details, see "PC-DMIS Vision Frame Grabber and Camera Setup".

- The factory has installed the device driver for CWS (required for a USB connection).