laser

#### Scan Zoom States (for CMS Sensors)

CMS sensors provide you with an additional area called Zoom, which is added to the bottom of the Laser Scan Properties tab of the Probe Toolbox. This area tells the sensor to work in predefined zoom states, with each state comprised of a specific combination of sensor frequency, data density, and Field of View (FOV) width.

Sample Zoom area

This area displays a table-like arrangement of option buttons arranged in columns and rows. Across the top, the "columns" show the data density. Along the side, the "rows" list the FOV width. You can only select proper combinations (those option buttons with a green background). Improper combinations are grayed out.

Hover your pointer over any valid option button to display the selected scan mode information in a yellow tooltip.

Sample tooltip under the mouse

Examples of CMS Scan Zoom States

Maximize your help viewer, and then click on the images below. Notice how different scan states change the display in the Laser tab:

4.1 Pts/mm and 124mm Width

8.4 Pts/mm and 60mm Width

16.8 Pts/mm and 24mm Width

Available Scan Zoom States for HP-L-20.8

Width (mm) | Density (Pts/mm)