core

### Using GD&T Selection Mode (from Capture)

This mode opens Snipping Tool from your operating system so that you can manually capture a single GD&T tolerance from the blueprint and use Optical Character Recognition (OCR) to import it.

While an OCR method is in use, DO NOT Copy or Cut information to the Clipboard, or you may lose that information.

This occurs because PC-DMIS monitors the Clipboard. If it detects something in the Clipboard, it assumes it's a GD&T tolerance, and it attempts to import it into PC-DMIS. When it tries to import the data it clears out the Clipboard.

If PC-DMIS cannot parse the information from the Clipboard, it shows an error message that says, "Cannot parse the selected note".

Procedure

1. Locate an electronic file or drawing that contains GD&T information. OCR detection works best with at least 300 DPI. Lower resolutions may produce less accurate results.

2. Open the image and position it next to PC-DMIS. For best results, use a separate monitor.

3. On the electronic file or drawing, zoom in close enough so that the text is at least 30 pixels tall. If the zoom level for the text isn't this tall, the OCR detection may produce less accurate results.

4. From the Graphic Modes toolbar or the QuickMeasure toolbar, click GD&T Selection Mode (from Capture) () to show Snipping Tool. (Snipping Tool is a screen capture utility that comes with your Windows operating system.)

3. From Snipping Tool, click New to start a new capture. The screen takes on a white overlay, and your pointer turns to a cross symbol.

4. On your electronic file, drag a rectangular box around the entire FCF.

5. Release the left mouse button to finish the capture. The Snipping Tool shows the capture, and after a few seconds, PC-DMIS shows the captured image inside the Selection Preview window, and the OCR widget appears.

6. Follow the instructions in the OCR widget to select features to define the GD&T tolerance. Use QuickFeatures to select the minimum number of features from the CAD model for the current step.

7. Once you define a feature or features from the CAD model for a step, from the widget, click Next (). This continues with the next step of the GD&T definition. That button becomes enabled once you've defined the minimum number of features.

8. Once you define the features and the widget informs you that the tolerances definition is completed, click Apply (). This accepts the changes made in the Edit window and closes the widget.

Best Practices

When you use this method, you need to be able to see both PC-DMIS and your electronic document at the same time. While it is possible to capture and convert a FCF on a single monitor, we recommend that you use two monitors.

OCR detection works best with an image that has at least 300 DPI. Lower resolutions may produce less accurate results.

Make the capture as clean as you can. It should be as close as possible to the FCF box in your electronic document. Exclude as much as you can from leader lines. Try not to capture extraneous information. Zoom in close enough so that the text is at least 30 pixels tall.

When you have imported the desired GD&T tolerances, check the FCF commands that PC-DMIS generated and make any needed corrections.

Related Topics:

About Optical Character Recognition (OCR) to Create FCFs

Using GD&T Selection Mode (from File)

OCR Selection Preview Window

OCR Widget