core

#### Clearance Plane Toggle

This icon lets you determine whether or not PC-DMIS inserts an automatic MOVE/CLEARPLANE command before measuring the first automatic hit of any auto features created after selecting the toggle icon.

In order to enable the Clearance Plane Toggle in the Auto Feature dialog, there are few prerequisites:

- The measurement routine needs to be set in a DCC mode (not manual)

- A clearance plane command needs to be in the measurement routine (press the F10 key on your keyboard and then click the Clearance Plane tab): CLEARP/ZPLUS,0,ZPLUS,0,OFF or CLEARP/ZPLUS,0,ZPLUS,0,ON)

The OFF/ON at the end of this command acts as the default for the toggle, each time you open a new Auto Feature dialog to create a new feature. This means that each time a new Auto Feature dialog is opened, the default for the toggle is the OFF/ON you have on the last CLEARP/ZPLUS,0,ZPLUS command. If you want to create an auto feature WITHOUT the Auto Feature dialog open (using the QuickFeature mode for example, with hovering – Shift+hover), the value for the toggle of the next QuickFeature is the last toggle you set in the dialog. This is why with QuickFeatures you don’t have control over this, while you can control it if the Auto Feature dialog is opened.

- If selected, PC-DMIS automatically inserts a MOVE/CLEARPLANE command (relative to the current coordinate system and part origin) into the Edit window before the first automatic hit of the feature. This causes the probe to move to the defined clearance plane before measuring the feature. After the last hit on the feature is measured, the probe will stay at probe depth until called to the next feature.

- If not selected, PC-DMIS creates Auto Features normally without inserting any MOVE/CLEARPLANE commands.

Using clearance planes reduces programming time because the need to define intermediate moves is reduced. It can also help protect your hardware from an inadvertent collision with the part. See "Parameter Settings: Clear Plane tab" in the "Setting your Preferences" chapter for additional information on Clearance Planes.

When measuring studs, be sure to set the spacer value to a distance that will allow the probe to move around the stud.

Move Clearance Plane Active Toggle

The default for the Clearance Plane toggle for all auto features is defined by the Clearance Plane Active toggle option (if defined) and is recalled whenever the Auto Feature dialog opens to create new features.