miim

#### COMMUNICATION

TcpipPort = 1294 Can be set in the setup dialog pane too –

TcpipIPAddress = 127.0.0.1 TCP/IP address of the server

2019 R1
Machine Interface Installation Manual

>> Back to Top

Contact the Documentation Team

PDF Documentation

>> Readme.pdf

>> Printable Manuals

Support Links

>> Knowledge Base ●

>> Hexagon Technical Support ●

>> Forum ●

>> Ideas ●

>> Training ●

>> Regional Offices ●

Company Information

Hexagon Manufacturing Intelligence

>> http://hexagonmi.com ●

Product Information

PC-DMIS 2019 R1

Copyright © 2019 Hexagon Manufacturing Intelligence – Metrology Software, Inc.

Help System last generated on 14 January 2019

>> http://www.pc-dmis.com ●