core

Step 1 - Select the LSPX1SF / HR-X (HR-X1-SF) Probe Changer

To select the LSPX1SF / HR-X (HR-X1-SF) Probe Changer:

1. Select the Type tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer).

2. In the Probe changer type list, select LSPX1SF / HR-X (HR-X1-SF):

Probe Changer dialog box - Type tab

3. To make this probe changer active and load the settings that apply to it, click Apply. Other tabs become visible after you click Apply.

4. In the Number of probe changers box, specify the number of probe changers that you want to define.

5. In the Active probe changer list, select the list item that represents the probe changer that you want to define. If this is the first probe changer, it appears as Probe Changer 1: TYPE=None.

6. In the Docking speed box, type a value. 15% is appropriate for this machine configuration.

FDC Controller Settings

If you are using an FDC controller, define your type of probe changer in the controller's common parameters as follows:

- Set changerType to 0 (where 0 = "others").

- Set X1ChangerType to 1.

B5 Leitz Controller Setting

If you are using a B5 Leitz controller, modify the controller's config file as follows:

TOOL_PORT_TYPE....: SHOPFL

Next Step

In the next step, you define the location your probe body moves to when using the probe changer to switch probe components.