miim

#### CWS.ini

Section | Key | Default Value | Type of Value | Description
COM | DEBUG | 0 | Integer | Enable debugging: Off = 0, On = 1
COM | Connected | 0 | integer | Connect to device: No = 0, Yes = 1
COM | Port | 7 | integer | Serial port number for CWS
COM | Baudrate | 115200 | integer | USB connection with CHROCODILES requires 921600
GRAPHIC | Range | 3.0 | Double | Measurement range of the connected sensor head
GRAPHIC | Zero | 50.0 | Double | Zero position [%] in the measurement range
CONFIG | SensorHeadNo | 0 | Integer | Sensor head number of the connected sensor head
CONFIG | ForceSensorHeadNo | 0 | Integer | Sensor head counting method: indexed with 0 = 0, indexed with 1 = 1
CONFIG | CHECKSINGLEVALUES | 1 | integer | Validate single point measurement raw result: validation off = 0, validation on = 1
Debug | FileTrace.System.Commands | 0 | integer | Log CWS system commands in HMV debug files: Off = 0, On = 1