core

#### Calibrating the SP600 Probe Changer

These topics describe how to define and calibrate the SP600 Probe Changer.

There are no inserts or extensions used for any of the port positions.

A Renishaw SP600 Stylus Change Rack (SCR600)

The SP600 Probe Changer DOES NOT need to be mounted on the machine table parallel to either the X or Y axis. For mounting instructions, consult the documentation that came with your probe changer.

To calibrate your probe changer:

Step 1 - Select the SP600 Probe Changer

Step 2 - Define the Mount Point

Step 3 - Prepare for Calibration

Step 4 - Take the First Manual Hit

Step 5 - Take the Second Manual Hit

Step 6 - Take the Third Manual Hit

Step 7 - Review the Calibration Results