miim

#### Move Parameters

BufferedMoves = TRUE - Boolean. The default is TRUE. If the value is FALSE, PC-DMIS waits for the move to complete before it sends the next move command. This registry entry is used only for diagnostic purposes.

ManSpeed = 100.0 - The speed in mm/s. The default is 100.0. The value sets the move speed when the machine goes from DCC mode to Manual mode since CMM-OS uses the last-received speed.

ManualMachineType = 0 - Integer. The default is 0 (zero). If the value is 1, you can only use manual machines.

MaxSpeed = 50.0 - The speed in mm/s. The default is 50.0. This registry entry calculates the percentage of the maximum speed since CMM-OS requires a percentage.

UseCircularMoves = TRUE - Boolean. The default is TRUE. This registry entry is a legacy entry. Do not change the value unless requested.

UseMZForMove = TRUE - Boolean value, the default is TRUE. This registry entry is a legacy entry. Do not change the value unless requested.