core

Recalibrate the Ports

After you complete a full calibration of the HR-MS (used with LSPX1) Probe Changer, you can choose to recalibrate all ports in DCC mode, or recalibrate a single port.

Recalibrating All Ports in DCC Mode

Recalibrating a Single Port

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.