miim

## Non-PWM Protocol

For details about testing the lights in a terminal for the non-PWM protocol, see "Testing the Lights in a Terminal".

ASCII Code | Keyboard Key (All letters are Lowercase) | Action
49 | 1 | Turns red lights ON, no flashing
50 | 2 | Turns yellow lights ON
51 | 3 | Turns green lights ON
52 | 4 | Turns white lights ON
53 | 5 | Turns blue lights ON
54 | 6 | (unused)
55 | 7 | Makes the LED fading speed 1 (fastest)
56 | 8 | Makes the LED fading speed 2
57 | 9 | Makes the LED fading speed 3
48 | 0 | Makes the LED fading speed 4 (default)
45 | - | Makes the LED fading speed 5
61 | = | Makes the LED fading speed 6 (slowest)
113 | q | Turns red lights OFF
119 | w | Turns yellow lights OFF
101 | e | Turns green lights OFF
114 | r | Turns white lights OFF
116 | t | Turns blue lights OFF
121 | y | Sets red lights flashing
117 | u | Sets yellow lights flashing
105 | i | Sets green lights flashing
111 | o | Sets white lights flashing
112 | p | Sets blue lights flashing
97 | a | (unused)
115 | s | (unused)
100 | d | (unused)
102 | f | (unused)
103 | g | (unused)
104 | h | (unused)
106 | j | (unused)
107 | k | (unused)
108 | l | (unused)
59 | ; | (unused)
122 | z | (unused)
120 | x | (unused)
99 | c | Sets 0 lights flashing
118 | v | (unused)
98 | b | (unused)
110 | n | (unused)