Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
ControlPoint Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : ControlPoint Object

Glossary Item Box

# Public Properties

Crossings | This defines the number of time the scan crosses the specified boundary before the alterations defined by the crossing point take effect.
I | This specifies the I component of the interrupt location's IJK vector.
J | This specifies the J component of the interrupt location's IJK vector.
K | This specifies the K component of the interrupt location IJK vector.
PointDensity | This defines the density of points per millimeter the scan shoud take after it encounters the control point.
PointDensity2 | Read/Write: Number of Points per MM for control point. Can be less than 1
Radius | This defines the Radius of circular control point types (Cones, Spheres, Cylinders).
Speed | Read/Write: Scan Speed Setting for control point
Type | This specifies the type of control point.
X | This specifies the X value of the interrupt XYZ location.
Y | This specifies the Y component of the interrupt XYZ location.
Z | This specifies the Z component of the interrupt XYZ location.

# See Also

ControlPoint Object

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.