miim

## TESASTAR-R

You can modify the following registry entries in the Option section of the PC-DMIS Settings Editor:

- TESASTAR-RClearance - This value specifies the clearance location directly in front of a given port of your TESASTAR-R probe changer. The default value is 50.

This clearance location value defines the distance in front of the port relative to the port center determined by the calibration. The probe moves to this location before it moves to the port for the drop-off or pickup.

Note that this value is used during the generation of motion for the change so that the value can be changed at any time without having to repeat the rack calibration.