miim

### Note on CW43L 3rd Axis Continuous C Joint

You can use the CW43L 3rd Axis Continuous C Joint with or without the CW43L probe changer.

If you are using the Continuous C Joint with the probe changer, you must set the following registry entries in PC-DMIS Settings Editor:

- HasContinuousCJoint - If the 3rd axis is in the probe changer, set the value to 0. If the 3rd axis is on the arm, set the value to 1.

- CW43LThirdAxisTCSlot = <port number>

If you are not using the CW43L probe changer, and you are using a Continuous C Joint, you must set the following registry entries:

- HasContinuousCJoint = 1

- CW43LThirdAxisTCSlot = -1