miim

### MP-169 Unexpected end-of-travel

Machine motion was prevented by a physical obstruction. Typically, this happens as a result of attempting to drive beyond the physical limits of one or more axes.

As a result, the machine is placed in Manual mode.

What you should do:

1. Determine the cause of the problem.

Remove the physical obstruction or correct the measurement routine.

2. If the problem persists when the machine motion is not obviously restricted:

You should contact your Giddings & Lewis service representative.