Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
BasicScan Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : BasicScan Object

Glossary Item Box

# Public Methods

AddControlPoint | Adds a control point to a scan.
CreateBasicScan | This method creates a basic scan object.
GenerateScan | Generates the points for the scan
GetBoundaryConditionParams | Gets the boundary condition parameters
GetBoundaryPoint | Returns the boundary point specified by the index
GetControlPoint | Returns the control point specified by the index.
GetFilterParams | Gets parameters used in filtering of scan data
GetHitParams | Gets parameters for the hit type used in the scan
GetHitTValue | Returns T deviation values for specified scansion hit
GetMethodParams | Gets the scan method parameters
GetMethodPointData | This method is provided as a shortcut to getting these commonly used scan parameters all at once.
GetNomsParams | Gets the parameters used in finding of scan nominals
GetParams | This method is provided as a shortcut to getting commonly used scan parameters all at once.
RemoveControlPoint | Removes a control point.
SetBoundaryConditionParams | Boolean value. Boolean returns true if the function succeeds, false if it fails.
SetBoundaryPoint | Sets a boundary point.
SetControlPoint | Sets a control point at the specified index.
SetFilterParams | This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetHitParams | This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetMethodParams | This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetMethodPointData | This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetNomsParams | This method is provided as a shortcut to set these commonly used scan parameters all at once.
SetParams | This method is provided as a shortcut to set these commonly used scan parameters all at once.

# Public Properties

AutoClearPlane | Determines whether auto clearance planes mode is on or off.
BoundaryCondition | Represents the boundary condition type.
BoundaryConditionAxisV | Represents the boundary condition axis vector. This vector is used as the axis of the Cylindrical and Conical BoundaryConditions.
BoundaryConditionCenter | Represents the boundary condition center. This Point is used by all Boundary Conditions and is the location of the Boundary Condition.
BoundaryConditionEndApproach | Represents the boundary condition end approach vector. This vector is used by all Boundary Conditions and is the Approach Vector of the Probe as it crosses the Boundary condition.
BoundaryConditionPlaneV | Represents the boundary condition plane vector. This vector is the normal vector of the Plane used by the Plane and OldStyle Boundary Conditions.
BoundaryPointCount | Indicates the number of boundary points to used in a patch scan.
DisplayHits | Determines whether hits of the scan are displayed in the Edit window or not.
Filter | Represents the filter type.
HitType | Represents the type of hit to use.
Method | Represents the method type for this scan.
MethodCutPlane | Represents the method’s cut plane vector.
MethodEnd | Represents the scan’s end point.
MethodEndTouch | Represents the method’s end touch vector.
MethodInitDir | Represents the method’s initial direction vector.
MethodInitTopSurf | Represents the initial Surface Vector for the Edge method.
MethodInitTouch | Represents the method’s initial touch vector.
MethodStart | Represents the scan’s start point.
NominalMode | Represents how to determine the nominal values for this scan.
OperationMode | Represents mode of operation of the scan.
SinglePoint | Determines whether single point mode is on or off.

# See Also

BasicScan Object | BasicScanCommand Property

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.