miim

### Note on CW43L 3rd Axis Continuous C Joint

You can use the CW43L 3rd Axis Continuous C Joint with and without the CW43L probe changer.

If you are using the Continuous C Joint with the probe changer, you must set the following registry entries:

- HasContinuousCJoint

- 0 – If the third axis is in the probe changer.

- 1 – If the third axis is on the arm.

- CW43LThirdAxisTCSlot = Port number

If you are not using the CW43L probe changer, and you are using a Continuous C Joint, you must set the following registry entries:

- HasContinuousCJoint = 1

- CW43LThirdAxisTCSlot = -1

For more information, see "Interface-Specific Options".