settingseditor

### CollisionMoveClearanceInMM

Defines the distance that the probe moves away from the part when it detects a collision while trying to move the probe to the next feature. PC-DMIS attempts to go directly to the next feature, but compensates for collisions by inserting clearance move commands. It continues this process until it defines a collision free path to the next feature.

Entry Name: CollisionMoveClearanceInMM

Entry Type: Real Number to specify distance in MM. The default value is 10.