miim

### Installation Information

When you install PC-DMIS with a portlock or an LMS license correctly configured for the FDC-SLC interface (SLC = Sensor and Light Controller), the correct files and registry entries are set up during the installation.

The license requires the following:

- Vision - Enabled

- Interface - Vision

- Vision Type - SLC DCC

- Laser Probe Type - If required, Mycrona WLS in case of CWS, and Mycrona TTL in case of TTL

The additional requirements are:

- Vision Frame Grabber should already be installed. For details, see "PC-DMIS Vision Frame Grabber and Camera Setup".

- The factory has installed the device driver for CWS (required for a USB connection).