miim

### Interface-Specific Options

FrameGrabber_Type - This setting defines the imaging hardware. Note that this is a decimal value.

This setting has these options:

Matrox CronosPlus = 2

Matrox Corona II = 5

IDS Falcon = 201

IDS Eagle = 202

IDS uEye = 203

National Instruments IMAQ = 301

FrameGrabber_CameraType - This setting defines the camera format type. Note that this is a decimal value.

This setting has these options:

NTSCYC = 0

PALYC = 1

NTSC = 2

PAL = 3

CCIR = 4 (monochrome)

CAMERA_USECFGFILE = 101

FrameGrabber_ConfigFile - This setting defines the frame grabber configuration file name. A configuration file name must be specified for camera types of 101.

FrameGrabber_LatchingMode - This setting defines the latching mode for specific systems. An example is a system with an FDC controller, which has hardware that supports the synchronization of an image frame capture and the stage position. For more details, see "Latching". Note that this is a decimal value.

This setting has these options:

No latching = 0

Frame grabber latching (Eagle) = 3

uEye camera latching = 24