core

#### Calibrating the TESASTAR-PR / HR-P Probe Changer

The calibration process for the TESASTAR-PR / HR-P Probe Changer represents the steps that you would take to prepare to use any of the probe changers that PC-DMIS supports. The process discussed here is specific to the TESASTAR-PR / HR-P Probe Changer.

No inserts or extensions are used for any of the port positions.

TESASTAR-PR / HR-P Probe Changer rack

The TESASTAR-PR / HR-P Probe Changer MUST be mounted on the machine table parallel to a machine axis, such as the X or Y axis. For mounting instructions, consult the documentation that came with your probe changer.

To calibrate your probe changer:

Step 1 - Select the TESASTAR-PR / HR-P Probe Changer

Step 2 - Define the Mount Point and Wrist Angle

Step 3 - Define the Number of Ports

Step 4 - Prepare for Calibration

Step 5 - Take the First Manual Hit

Step 6 - Take the Second Manual Hit

Step 7 - Take the Third Manual Hit

Step 8 - Review the Calibration Results