Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
BSBOUNDCOND_ENUM Enumeration
See Also Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : BSBOUNDCOND_ENUM Enumeration

Glossary Item Box

# Members

Member | Value | Description
--- | --- | ---
BSBOUNDCOND_CONE | 600050 | Represents a Conical Boundary Condition. This Boundary condition requires the following parameters to be set you user using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, BoundaryConditionAxisV, HalfAngle, number of Crossings.
BSBOUNDCOND_CYLINDER | 600040 | Represents a Cylindrical Boundary Condition. This Boundary condition requires the following parameters to be set by you using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, BoundaryConditionAxisV, Diameter, number of Crossings.
BSBOUNDCOND_PLANECROSS | 600030 | Represents a Planar Boundary Condition. This Boundary condition requires the following parameters to be set by you using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, BoundaryConditionPlaneV, number of Crossings.
BSBOUNDCOND_SPHERE | 600010 | Represents a Spherical Boundary Condition. This Boundary condition requires the following parameters to be set by you using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, Diameter, number of Crossings.

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.