miim

### Geometric Error Compensation (VOLCOMP)

It’s anticipated that most people using this PC-DMIS interface will use the normal LK VolComp option, which simply means the interface will not do any VolComp adjustments itself and will leave it up to the driver. In that mode, VolComp may or may not be utilized depending on the common driver configuration.

This interface does provide the option of enabling other VolComp methods. If using one of those VolComp methods, it is highly recommended that you make sure the error correction is turned off in the common driver configuration.

Leave VolCompMethod at its default value of 0 to use the native LK VolComp configuration of the common driver.