laser

#### Setting Boundary Points Using the Measured Point Method

To set the boundary of the scan using measured points:

1. Place the laser sensor at the desired location.

2. On the jog box, press the Probe Enable button (only available on DEA and Brown and Sharpe machines).

- This automatically updates the value of the selected boundary point in the Boundary Points and Vectors list. The software then selects the next boundary point (if any) in the list.

- In the case of a PATCH scan, PC-DMIS adds an extra boundary point automatically if the selected point is the last point in the list. The PATCH scan displays the last point (this is the same as the previous point). PC-DMIS deletes this last point when you click the OK button.

The Probe Enable light on the jog box alternates between off and on every time you press the Probe Enable button. This is not important and has no influence on the probe itself.