portable

## Probe Trigger Options

Probe trigger options allows you to trigger a hit when certain conditions are met while you use manual CMM machines.

The interfaces that support probe trigger options include Romer, Leica, Faro, Garda, and SMX Laser.

You can insert POINT AUTOTRIGGER, PLANE AUTOTRIGGER, and POINT MANUAL TRIGGER commands into your measurement routine from the Probe Trigger Options tab in the Parameters dialog box (Edit | Preferences | Parameters or F10) or from the Probe Mode toolbar.

These trigger commands function with the following features:

- Auto Features: Circle, Ellipse, Edge Point, Round Slot, Square Slot, Notch Slot, and Polygon

- Measured Features: Circle, Line, and Round Slot

The probe trigger options are:

- Point AutoTrigger

- Plane AutoTrigger

- Point Manual Trigger