planner

## The Status Bar

The status bar displays the following:

1. Message Box: The left-most box displays instructions and other information regarding the current procedure or command.

2. X, Y, and Z boxes: These boxes show the X, Y, and Z position of the probe. Clicking on any of the three coordinate displays within the status bar will cause the Auto Move Point dialog box to appear. (See "Inserting a Move Point Command" in the "Inserting Move Commands" chapter for additional information regarding DCC Move Point.)

3. W: Angle of Rotary Table.

4. A, B, and C boxes: These boxes show the A, B, and C wrist angles for a three-axis wrist probe such as a CMS probe. Your wrist probe may only support two axes. In that case, this portion of the status bar only shows A and B.

5. SD: This shows the standard deviation of the last feature measured.

6. # of Hits: This shows the number of hits currently taken.

7. IN/MM: This shows the current unit of measurement used for the measurement routine.

8. Line: This box displays a number that indicates the current line where the cursor is located in the Edit report. Col: This text displays a number that indicates the current column where the cursor is located in the Edit report.

Status Bar Manipulations

- To increase the size of the status bar, select View | Status Bar | Large. Due to its increased size, this large status bar only displays the Message, the XYZ , the SD, the # of Hits:, the Line:, and the Col: boxes.

- To put the status bar back to its normal size, select View | Status Bar | Normal.

- To hide or show the status bar, select View | Status Bar | Hide Status Bar(s).