miim

### Interface-Specific Options

To set the values for registry entries for the FDC-VisionBox Interface, use the PC-DMIS Settings Editor.

Registry Entry | Default Value |  | Settings Editor Section
IlluminationConfiguration | 0 | Autodetect = 0, Optive321 = 1 | VisionBox
OpticsDeadband | 100 |  | VisionBox
StageSettleTime | 0.25 |  | VisionBox
TcpipIPAddress | 192.168.3.9 |  | VisionBox
TcpipPort | 1234 |  | VisionBox

Laser (CWS or TTL) requires different setups. For CWS, you need to set these registry entries:

Registry Entry | Default Value | Settings Editor Section
CWSPresent | TRUE | FDC
Laser_Type | 2 | MSI

For TTL, you need to set these registry entries:

Registry Entry | Default Value | Settings Editor Section
FLSPresent | TRUE | FDC
Laser_Type | 1 | MSI

If you install a rotary table, you need to set these additional settings:

Registry Entry | Default Value | Settings Editor Section
EnableRotaryAbsolutePosition | TRUE | FDC
EnableRotaryClockMode | TRUE | FDC
SendHSSFullData | 2 | FDC
RotaryMinDelta | 0.05 | FDC
RotaryOffset | 0 | FDC
RotaryOffsetSpeed | 50 | FDC
RotaryTablePresent | TRUE | FDC