core

#### Calibrating the TP20 Probe Changer

The calibration process for the TP20 Probe Changer represents the steps that you would take to prepare for using any of the probe changers that PC-DMIS supports. The process in this documentation is specific to the TP20 Probe Changer.

No inserts or extensions are used for any of the port positions.

TP20 Probe Changer rack

The TP20 Probe Changer does not need to be mounted on the machine table parallel to a machine axis, such as the X or Y axis. For mounting instructions, consult the documentation that came with your probe changer.

To calibrate your probe changer:

Step 1 - Select the TP20 Probe Changer

Step 2 - Define the Mount Point and Wrist Angle

Step 3 - Define the Number of Ports

Step 4 - Prepare for Calibration

Step 5 - Take the First Manual Hit

Step 6 - Take the Second Manual Hit

Step 7 - Take the Third Manual Hit

Step 8 - Review the Calibration Results