laser

#### Edge Point Command Mode Text

The Edge Point command inside the Edit window’s Command Mode looks like this:

PNT2 =FEAT/LASER/EDGE POINT,CARTESIAN

THEO/<1.895,1.91,1>,<0,1,0>,<0,0,1>

ACTL/<1.895,1.91,1>,<0,1,0>,<0,0,1>

TARG/<1.895,1.91,1>,<0,1,0>,<0,0,1>

SHOW FEATURE PARAMETERS=YES

SURFACE1=THEO_THICKNESS,1

SURFACE2=THEO_THICKNESS,0

MEASURE MODE=NOMINALS

RMEAS=NONE,NONE,NONE

AUTO WRIST=NO

GRAPHICAL ANALYSIS=NO

FEATURE LOCATOR=NO,NO,""

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

SENSOR FREQUENCY=25,OVERSCAN=2,EXPOSURE=18

FILTER=NONE