miim

### RCU-707 RCU EPROM B checksum error

There is a checksum error in EPROM at board position F10.

For more information, see "RCU Error Codes".

What you should do:

1. Note the display on the MP.

2. To clear the error, power the MP down.

3. Power the MP back up.

4. Reseat the 2716 chip at board position F10.

5. If the error reoccurs, contact your Giddings & Lewis service representative.