miim

### Sample mv_config.cfg File

;

; This file must be located in the PC-DMIS directory with pcdlrn.exe to be processed

; Comment lines must have a; as the first character

; To use a command, delete the; at the start of the line

;

; Set the scale resolution in mm. The hard-coded default is 0.0005

;

SCALE_RESOLUTION_X 0.0005

SCALE_RESOLUTION_Y 0.0005

SCALE_RESOLUTION_Z 0.0005

;

; Set the move settle time maximum wait time in milliseconds

;

EDGE_RETRY_TIMEOUT_X 800

EDGE_RETRY_TIMEOUT_Y 800

EDGE_RETRY_TIMEOUT_Z 800

EDGE_RETRY_TIMEOUT_MAG 800

;

; distance to destination in scale counts for move to be judged completely

;

EDGE_RETRY_BANDWIDTH_X 1

EDGE_RETRY_BANDWIDTH_Y 1

EDGE_RETRY_BANDWIDTH_Z 1

EDGE_RETRY_BANDWIDTH_MAG 1

;

; Size of the zoom backlash move to ensure zoom cell repeatability regards of the last move direction

; This value is read from the machine controller

;

ZOOMBACKLASHMOVE 300

;

; illumination settle time to ensure that the illumination is set and stable before measurement is done

;

ILLUMINATIONSETTLETIME 50

;

;ROTARY=1

TOUCH_PROBE=1

;

;Test Auto retract setting

;

MANUAL_RETRACT_SPEED 6.0

; LOGINIT = 0x0001 Log machine initialization

; LOGACTIONS = 0x0002 Log command actions

; LOGCOMM = 0x0004 Log communication (file grows rapidly)

; LOGFLUSH = 0x0008 Close/open file on every write to grab info before crash

; full logging without flushing would be 1 + 2 + 4 or 7

DEBUG 0