settingseditor

### DccAngleExterior

Defines the angle as either interior or exterior. Interior angles have the solid angle of the part less than 180°, while exterior angles are greater than 180°. With the exterior option enabled, PC-DMIS will measure the angle as exterior.

Make sure this option is set correctly because of the differences in measurement sequence for each type.

Entry Name: DccAngleExterior

Entry Type: Whole Number to specify Exterior(1) or Interior(0) angle. The default value is 1.