miim

### MLB-162 APC rack could not be raised

A command was executed, which required that the APC rack be raised, and it could not be raised.

As a result, the command is not executed.

What you should do:

1. Check the command's definition and correct the measurement routine.

2. Correct the problem with the APC racks lower/raise capability.

3. If the error reoccurs, contact your Giddings & Lewis service representative.