core

Step 3 - Define the Number of Ports

The final step prior to the actual calibration of the TESASTAR-PR / HR-P Probe Changer is to define the number of ports on the probe changer.

To define the number of ports:

1. Select the Ports tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer):

Probe Changer dialog box - Ports tab

2. In the Active probe changer list, select TYPE=TESASTAR-PR.

3. In the Number of ports box, type the number of ports that you want to define. This should match the number of physical ports on the probe changer.

4. To save your changes, click Apply.

The next step starts the calibration process.