core

#### Procedure 3: Finding Nominal Points on All CAD Surfaces

If PC-DMIS still cannot find a valid nominal point by using the procedures discussed in procedures 1 and 2, (see the "Procedure 1: Finding Nominal Points on the Previous Surface" and "Procedure 2: Finding Nominal Points on Priority Surfaces" topics), it does the following:

- Looks for the best nominal point on all the CAD surfaces within the FindNoms tolerance

- Creates an Auto Vector Point based on the best available nominal point.

- Displays all the CAD surfaces that had nominal points in the FindNoms Override dialog box.