core

### Parameter Settings: Probe Trigger Options tab

Parameter Settings dialog box - Probe Trigger Options tab

The Probe Trigger Options tab allows you to determine tolerance zones and then insert POINT AUTOTRIGGER, PLANE AUTOTRIGGER, and POINT MANUAL TRIGGER commands into the Edit window. These commands trigger a hit when certain conditions are met.

Only manual CMM machines with certain interfaces support these probe trigger options. These interfaces include Faro, Romer, Garda, Leica, Polar, and SMXLaser.

To access this tab:

1. Select Edit | Preferences | Parameters to display the Parameter Settings dialog box.

2. Select the Probe Trigger Options tab.

Supported Features

These trigger commands function with these supported features:

- Auto Features: Circle, Ellipse, Edge Point, Round Slot, Square Slot, Notch Slot, and Polygon

- Measured Features: Circle, Line, and Round Slot

In addition, the POINT AUTOTRIGGER command supports the Auto Vector Point and Measured Point features.

More:

Point AutoTrigger area

Plane AutoTrigger area

Point Manual Trigger area