laser

### Exposure and Gray Sum Settings by Feature and Material

Based on the feature type and the part material type the Exposure value found on the Laser Scan Properties tab and the Min and Max Gray Sum values found on the Laser Pixel CG Locator Properties tab should be adjusted according to the following table:

Exposure and Gray Sum Settings
Feature Based
Feature | Material | Exposure | Min Grey Sum | Max Grey Sum
Sphere | Tungsten Calibration Sphere | 120 | 10 | 300
Ceramic | 80 | 10 | 300
Gap/Flush | Sheet Metal | 150 | 30 | 300
White | 100 | 30 | 300
Blue | 120 | 30 | 300
Black | 450 | 10 | 300
Circle | Sheet Metal | 100 | 50 | 300
White | 100 | 50 | 300
Blue | 120 | 50 | 300
Black | 450 | 30 | 300
Aluminum | 80 | 50 | 300
Slot | Sheet Metal | 100 | 50 | 300
White | 100 | 50 | 300
Blue | 120 | 50 | 300
Black | 450 | 30 | 300
Aluminum | 80 | 50 | 300
Edge Point | Sheet Metal | 100 | 50 | 300
White | 100 | 50 | 300
Blue | 120 | 50 | 300
Black | 450 | 30 | 300
Aluminum | 80 | 50 | 300
Plane | Sheet Metal | 100 | 30 | 300
White | 100 | 30 | 300
Blue | 120 | 30 | 300
Black | 450 | 10 | 300
Aluminum | 80 | 30 | 300
Surface Point | Sheet Metal | 100 | 30 | 300
White | 100 | 30 | 300
Blue | 120 | 30 | 300
Black | 450 | 10 | 300
Aluminum | 80 | 30 | 300

Exposure and Gray Sum Settings