core

Step 6 - Take the Second Manual Hit

For the LSPX1C / HR-X (HR-X1-P) Probe Changer, take the second manual hit in the XY plane on the front left side of the first port. The prompt for the second hit on the front surface of the first port is:

PC-DMIS Message

Please take a hit on the front surface on the left side of the first port (port 1). Be careful to avoid the tapered corner and take the hit on the flat portion.

Prompt for the second manual hit on the front surface of the first port

1. When you are ready to take the second measurement, click OK.

2. Use your machine's jog box to measure the second hit on the front left face of the first port as shown below:

View of the second hit on the front left face of the first port

In the next step, you take manual hits on the top of each port.