miim

### Multiple uEye Digital Cameras

You can use multiple uEye digital cameras. To do this, you must set the camera IDs in the IDS Camera Manager. The camera IDs must be sequential and start with 1. The configuration file name must denote the number of cameras installed. The uEye Camera ID and the PCDMIS vision probe ID are offset by 1. For example, if the camera has an ID of 1, the PC-DMIS Vision probe sees it as a camera with the ID of 0.

You must configure the cameras for the same color depth and resolution. (for example, 8 bit monochrome vs 32 bit color, 1280 x 1024 vs 768 x 576, etc.)