settingseditor

### AdjacentEdgeToleranceInMM

This option is used to eliminate internal borders between surfaces for determining edges. This is useful in situations where the CAD model has gaps between surfaces. If the gaps are large, you may need to increase the default value of 0.1MM.

Entry Name: AdjacentEdgeToleranceInMM

Entry Type: Real Number specifying tolerance. The default value is 0.1.