core

Step 5 - Take the Second Manual Hit

For the SP600 Probe Changer, you will take the second manual hit in the Z direction, on the horizontal face on top of the rack between port 2 and port 3.

The prompt for the second hit on the top is:

PC-DMIS Message

Please take a hit on top of the metallic docking plate in the middle between ports 2 and 3.

Use your machine's jog box to measure the second hit on the top metal surface between port 2 and port 3.

In the next step, you take the third manual hit.