miim

#### ZEISSTC1 (supported)

This probe changer is generally used on machines with the ST2 or ST3 switching probe head. It is not used on machines with a scanning probe head. Refer to the general probe changer setup section for how to enable this type of probe changer in PC-DMIS. The probe changer type must be defined as ZEISSTC1. See the ToolChangers.doc document for specific details on using and configuring toolchangers.